Menu

- Learn
- Documentation
  - Language Reference
  - Library Reference
  - Command-line Reference
  - Feature Overview
  - Articles
- Downloads
- Packages
- Community
  - Blog
  - Orgs using D
  - Twitter
  - Forums
  - IRC
  - Community Discord
  - Wiki
  - GitHub
  - Issues
  - Get involved
  - Contributors
  - Foundation
  - Security Team
  - Donate
  - Sponsors
- Resources
  - Tour
  - Books
  - Tutorials
  - Tools
  - Editors
  - IDEs
  - run.dlang.io
  - Visual D
  - Acknowledgments
  - D Style
  - Glossary
  - Sitemap

Search
Report a bug
If you spot a problem with this page, click here to create a Bugzilla issue.
Improve this page
Quickly fork, edit online, and submit a pull request for this page. Requires a signed-in GitHub account. This works well for small changes. If you'd like to make larger changes you may want to consider using a local clone.

# core.simd

Builtin SIMD intrinsics

Source core/simd.d

License:
Boost License 1.0.
Authors:
Walter Bright,

Source core/simd.d

template `Vector`(T)
  Create a vector type.

  Parameters T = one of double[2], float[4], void[16], byte[16], ubyte[16], short[8], ushort[8], int[4], uint[4], long[2], ulong[2]. For 256 bit vectors, one of double[4], float[8], void[32], byte[32], ubyte[32], short[16], ushort[16], int[8], uint[8], long[4], ulong[4]

alias `void16` = __vector(void[16]);
alias `double2` = __vector(double[2]);
alias `float4` = __vector(float[4]);
alias `byte16` = __vector(byte[16]);
alias `ubyte16` = __vector(ubyte[16]);
alias `short8` = __vector(short[8]);
alias `ushort8` = __vector(ushort[8]);
alias `int4` = __vector(int[4]);
alias `uint4` = __vector(uint[4]);
alias `long2` = __vector(long[2]);
alias `ulong2` = __vector(ulong[2]);
enum `XMM`: int;
  XMM opcodes that conform to the following:
  opcode xmm1,xmm2/mem
  and do not have side effects (i.e. do not write to memory).
  `STOSS`
    MOVSS xmm1/m32, xmm2
  `STOSD`
    MOVSD xmm1/m64, xmm2
  `STOAPS`
    MOVAPS xmm2/m128, xmm1
  `STOAPD`
    MOVAPD xmm2/m128, xmm1
  `STODQA`
    MOVDQA xmm2/m128, xmm1
  `STOD`
    MOVD reg/mem64, xmm 66 0F 7E /r
  `STOQ`
    MOVQ xmm2/m64, xmm1
  `LODSS`
    MOVSS xmm1, xmm2/m32
  `LODSD`
    MOVSD xmm1, xmm2/m64
  `LODAPS`
    MOVAPS xmm1, xmm2/m128
  `LODAPD`
    MOVAPD xmm1, xmm2/m128
  `LODDQA`
    MOVDQA xmm1, xmm2/m128
  `LODD`
    MOVD xmm, reg/mem64 66 0F 6E /r
  `LODQ`
    MOVQ xmm1, xmm2/m64
  `LODDQU`
    MOVDQU xmm1, xmm2/mem128 F3 0F 6F /r
  `STODQU`
    MOVDQU xmm1/mem128, xmm2 F3 0F 7F /r
  `MOVDQ2Q`
    MOVDQ2Q mmx, xmm F2 0F D6 /r
  `MOVHLPS`
    MOVHLPS xmm1, xmm2 0F 12 /r
  `LODHPD`
    MOVHPD xmm1, m64
  `STOHPD`
    MOVHPD mem64, xmm1 66 0F 17 /r
  `LODHPS`
    MOVHPS xmm1, m64
  `STOHPS`
    MOVHPS m64, xmm1
  `MOVLHPS`
    MOVLHPS xmm1, xmm2
  `LODLPD`
    MOVLPD xmm1, m64
  `STOLPD`
    MOVLPD m64, xmm1
  `LODLPS`
    MOVLPS xmm1, m64
  `STOLPS`
    MOVLPS m64, xmm1
  `MOVMSKPD`
    MOVMSKPD reg, xmm
  `MOVMSKPS`
    MOVMSKPS reg, xmm
  `MOVNTDQ`
    MOVNTDQ m128, xmm1
  `MOVNTI`
    MOVNTI m32, r32
  `MOVNTPD`
    MOVNTPD m128, xmm1
  `MOVNTPS`
    MOVNTPS m128, xmm1
  `MOVNTQ`
    MOVNTQ m64, mm
  `MOVQ2DQ`
    MOVQ2DQ
  `LODUPD`
    MOVUPD xmm1, xmm2/m128
  `STOUPD`
    MOVUPD xmm2/m128, xmm1
  `LODUPS`
    MOVUPS xmm1, xmm2/m128
  `STOUPS`
    MOVUPS xmm2/m128, xmm1
pure nothrow @nogc @safe void16 `__simd`(XMM `opcode`, void16 `op1`, void16 `op2`);
  Generate two operand instruction with XMM 128 bit operands.
  This is a compiler magic function - it doesn't behave like regular D functions.

  Parameters opcode = any of the XMM opcodes; it must be a compile time constant op1 = first operand op2 = second operand

  Returns:
  result of opcode

  Example

      import core.simd;
      import core.stdc.stdio;

      void main()
      {
          float4 A = [2.34f, -70000.0f, 0.00001f, 345.5f];
          float4 R = A;
          R = cast(float4) __simd(XMM.RCPSS, R, A);
          printf("%g %g %g %g\n", R.array[0], R.array[1], R.array[2], R.array[3]);
      }

  Prints 0.427368 -70000 1e-05 345.5. The use of the two operand form for XMM.RCPSS is necessary because the result of the instruction contains elements of both operands.

  Example

      double[2] A = [56.0, -75.0];
      double2 R = cast(double2) __simd(XMM.LODUPD, *cast(double2*)A.ptr);

  The cast to double2* is necessary because the type of *A.ptr is double.
  Examples:

      float4 a;
      a = cast(float4)__simd(XMM.PXOR, a, a);

pure nothrow @nogc @safe void16 `__simd`(XMM `opcode`, void16 `op1`);
  Unary SIMD instructions.
pure nothrow @nogc @safe void16 `__simd`(XMM `opcode`, double `d`);
pure nothrow @nogc @safe void16 `__simd`(XMM `opcode`, float `f`);
  Examples:

      float4 a;
      a = cast(float4)__simd(XMM.LODSS, a);

pure nothrow @nogc @safe void16 `__simd`(XMM `opcode`, void16 `op1`, void16 `op2`, ubyte `imm8`);
  For instructions: CMPPD, CMPSS, CMPSD, CMPPS, PSHUFD, PSHUFHW, PSHUFLW, BLENDPD, BLENDPS, DPPD, DPPS, MPSADBW, PBLENDW, ROUNDPD, ROUNDPS, ROUNDSD, ROUNDSS

  Parameters opcode = any of the above XMM opcodes; it must be a compile time constant op1 = first operand op2 = second operand imm8 = third operand; must be a compile time constant

  Returns:
  result of opcode
  Examples:

      float4 a;
      a = cast(float4)__simd(XMM.CMPPD, a, a, 0x7A);

pure nothrow @nogc @safe void16 `__simd_ib`(XMM `opcode`, void16 `op1`, ubyte `imm8`);
  For instructions with the imm8 version: PSLLD, PSLLQ, PSLLW, PSRAD, PSRAW, PSRLD, PSRLQ, PSRLW, PSRLDQ, PSLLDQ

  Parameters opcode = any of the XMM opcodes; it must be a compile time constant op1 = first operand imm8 = second operand; must be a compile time constant

  Returns:
  result of opcode
  Examples:

      float4 a;
      a = cast(float4) __simd_ib(XMM.PSRLQ, a, 0x7A);

pure nothrow @nogc @safe void16 `__simd_sto`(XMM `opcode`, void16 `op1`, void16 `op2`);
  For "store" operations of the form: op1 op= op2 such as MOVLPS.
  Returns:
  op2 These cannot be marked as pure, as semantic() doesn't check them.
pure nothrow @nogc @safe void16 `__simd_sto`(XMM `opcode`, double `op1`, void16 `op2`);
pure nothrow @nogc @safe void16 `__simd_sto`(XMM `opcode`, float `op1`, void16 `op2`);
pure nothrow @nogc @safe void16 `__simd_sto`(XMM `opcode`, void16 `op1`, long `op2`);
  Examples:

      void16 a;
      float f = 1;
      double d = 1;

      cast(void)__simd_sto(XMM.STOUPS, a, a);
      cast(void)__simd_sto(XMM.STOUPS, f, a);
      cast(void)__simd_sto(XMM.STOUPS, d, a);

void `prefetch`(bool writeFetch, ubyte locality)(const(void)* `address`);
  Emit prefetch instruction.
  Parameters:

  const(void)* `address` | address to be prefetched
  writeFetch | true for write fetch, false for read fetch
  locality | 0..3 (0 meaning least local, 3 meaning most local)

  Note The Intel mappings are:

  writeFetch | locality | Instruction
  --- | --- | ---
  false | 0 | prefetchnta
  false | 1 | prefetch2
  false | 2 | prefetch1
  false | 3 | prefetch0
  true | 0 | prefetchw
  true | 1 | prefetchw
  true | 2 | prefetchw
  true | 3 | prefetchw

V `loadUnaligned`(V)(const V* `p`)
if (is(V == void16) || is(V == byte16) || is(V == ubyte16) || is(V == short8) || is(V == ushort8) || is(V == int4) || is(V == uint4) || is(V == long2) || is(V == ulong2) || is(V == double2) || is(V == float4));
  Load unaligned vector from address. This is a compiler intrinsic.
  Parameters:

  V* `p` | pointer to vector

  Returns:
  vector
V `storeUnaligned`(V)(V* `p`, V `value`)
if (is(V == void16) || is(V == byte16) || is(V == ubyte16) || is(V == short8) || is(V == ushort8) || is(V == int4) || is(V == uint4) || is(V == long2) || is(V == ulong2) || is(V == double2) || is(V == float4));
  Store vector to unaligned address. This is a compiler intrinsic.
  Parameters:

  V* `p` | pointer to vector
  V `value` | value to store

  Returns:
  value

Copyright © 1999-2023 by the D Language Foundation | Page generated by Ddoc on Fri Sep 15 21:13:22 2023